물품규격 확인서

입찰공고번호	견적 2505-2호		입찰명		임피던스 분석기 구매
상호			대표자				(인)
담당자	성명			부서/직위
	휴대폰			이메일

품목번호	입찰공고 물품 규격 (수량)	제안 물품 규격 (수량)	공고규격 동일 여부	비고
1	임피던스 분석기 (1대)	* 제조사 : * 모델명 :	Y / N
	DC to 5MHz Frequency range, 1 mΩ to 1 TΩ Impedance Z range 0.05% basic accuracy at a rate of 20 ms/data point LabOne® Sweeper for frequency, bias voltage and test signal amplitude response measurements Compensation Advisor and Confidence Indicator for accurate measurements 25 s start-up time and high repeatability APIs for C, MATLAB®, LabVIEW®, Python, .NET Full MFLI lock-in amplifier functionality: time constants from 336 ns to 83 s Compatibility with MFITF test fixture Frequency resolution : 1 μHz Basic accuracy : 0.05% (1 mHz to 500 kHz) Basic temp. stability : <200 ppm/K Test signal level : 0 V to 2.1 Vrms, incl. monitoring Bandwidth : 276 μHz to 206 kHz DC bias signal level : 2T: ±10 V, 4T: ±3 V Compensation : SO, SOL, LLL, SL, L, OL Impedance Z : 1 mΩ to 1 TΩ, 0.05% Admittance Y : 100 pS to 1 kS, 0.05% Voltage V : 0 V to 3 V, 1% Current I : 0 mA to 10 mA, 2% Phases ϴZ,ϴY, ϴV, ϴI : ±180 deg, 10 μdeg resolution Resistance Rs, Rp : 1 mΩ to 1 TΩ, max(10 μΩ, 0.05%) Capacitance Cs, Cp : 10 fF to 1 F, max(10 fF, 0.05%)¹ Inductance Ls, Lp : 100 nH to 1 H, max(10 nH, 0.05%)¹ DC Resistance RDC : 1 mΩ to 1 TΩ, 2% Reactance X : 1 mΩ to 1 TΩ, 0.05% Conductance G, Susceptance B : 1 nS to 1 kS, max(100 nS, 0.05%) Loss coefficient D : 10-5 to 100’000 Q factor : 10-5 to 100’000 Sweep parameters : frequency, test signal amplitude, bias voltage, etc. Sweep points : 2 to 100’000 Sweep resolution : arbitrary, defined by start value, stop value and number of sweep points Sweep modes : sequential, binary, bidirectional, reverse Sweep step modes : linear, logarithmic Sweep speed : 20 ms/pt for f > 10 kHz LabOne toolset : Numerical view, Spectrum Analyzer, Plotter, Data Acquisition, Oscilloscope Confidence Indicator : suppression, compensation, open, underflow, overflow ※ 참조모델 : Zurich Instruments MFIA 5M	o o o

※ 물품규격 확인서 작성 유의사항

* 입찰공고된 규격 기준과 일치하는 품목으로 구성되어야 함

- 공고된 규격 기준과 동일한 경우 ‘공고규격과 동일 여부’ 표기

* 입찰서 제출시 본 물품규격 확인서를 반드시 첨부해야 함

- 규격 확인에 필요한 카탈로그, 제품사양서, 제작시방서, 도면, 사진이나 그 밖에 규격 검토에 필요한 증빙서류 포함

* 단종 등 불가피한 사유로 규격을 변경하여 제안하려는 경우에는 규격·품질·성능이 동등 이상인 품목으로 하며, 비고란에 사유를 명시

- 수요부서의 규격 확인에 필요한 카탈로그, 제품사양서, 제작시방서, 도면, 사진이나 그 밖에 규격 검토에 필요한 증빙서류를 제시하여 수요부서에 사전 입증·확인받아야 함

* 품목별로 구분하여 작성하며, 규격 검토자가 제안물품에 대해 알 수 있도록 주장비, 주변장비 및 부속품 등의 품명, 제조사, 모델명, 규격, 수량, 성능, 특징, 장단점, 제품인증 여부, 하자보증 및 A/S조건 등을 명시

* 수요부서의 물품규격 및 증빙서류 확인 결과, 동등 이상으로 인정되지 않는 경우에는 낙찰 후라도 선정을 취소하며, 입찰자는 이에 대한 이의를 제기할 수 없음