입찰규격 확인서

입찰공고번호	항대 26-10호	입찰명	세스나 단발항공기 엔진오일 물품구매
상호		대표자		(인)

담당자	성명		부서/직위
	휴대폰		이메일

수요부서 확인

(제주비행훈련원)

성명:

(인)

수요부서 확인자 의견

※ 입찰서 제출시 수요부서에 확인받은 본 입찰규격 확인서를 반드시 첨부해야 함

- 첨부하지 않거나 수요부서 확인이 누락된 경우 낙찰대상에서 배제

품목번호

입찰공고 물품 규격 (수량)

제안 물품 규격 (수량)

공고규격 동일 여부

비고

1

2

3

AEROSHELL W15W-50

* 제조사 :

* 모델명 :

Y / N

Y / N

Y / N

Specifications, Approvals

& Recommendations

• SAE J1899 Multigrade

• AMOC FAA AD 80-04-03 R2 p. 1b

AeroShell Oil W 15W-50 was developed in co-operation with Textron Lycoming and Continental Motors and conforms to their specifications 301F and MHS-24A respectively. This oil is also approved under Military Specification MIL-L-22851 which is now obsolete and has been replaced by the SAE J1899 specification. AeroShell Oil W 15W-50 is also approved for use in all Pratt & Whitney radial aircraft engines.

In addition AeroShell Oil W 15W-50 meets the provisions of Lycoming Service Bulletin 446C and 471, plus Service Instruction 1409A and meets the American FAA Airworthiness Directive 80-04-03 R2 p. 1b which specifies special anti-wear requirements for certain engine models.

• AeroShell Oil W 15W-50 already contains, in the correct proportions, an anti-wear additive equivalent to the Lycoming additive LW 16702; operators who use AeroShell Oil W15W-50 DO NOT need to add this Lycoming additive to the oil.

• AeroShell Oil W 15W-50 is qualified for use in all Continental Motors' liquid cooled and air cooled aircraft piston engines.

• French: XO-162/a3

• Joint Service Designation: OMD-162

• Textron Lycoming: 301F Service Bulletins 446C and 471, Service Instruction 14909A

• Continental: MHS 24A, SIL 99-2

• Pratt & Whitney: Service Bulletin 1183

Typical Physical Characteristics

o

o

o

o

AEROSHELL W100 Plus

* 제조사 :

* 모델명 :

Specifications, Approvals

& Recommendations

AeroShell Oil W100 Plus is a single grade oil that merges the ashless dispersant qualities of AeroShell Oil W100 and the anti-wear and anti-corrosion additives of AeroShell Oil W 15W-50 multigrade. Ideal for pilots who prefer a single grade oil but seeking for enhanced¹ engine protection and performance.

Country / OEM	Specification
SAE	J1899 Grade 50
FAA	AMOC to Airworthiness Directive 80-04-03 R2 p.1b
Lycoming Engines	Service Bulletin 446E and 471B Service Instruction 1409C
Continental Aerospace Technologies	MHS-24 SIL 99-2

Applications

The advanced additives in AeroShell Oil W100 Plus provide better rust and wear protection than conventional single grades. The additives work as a protective barrier to prevent critical parts from being slowly degraded by rust or wear, especially when an aircraft sits idle. This protection helps keep the camshaft and lifters coated, reducing the likelihood of premature damage and helping operators reach TBO.

Additional information

Advice on applications not covered here may be obtained from your Shell representative.

Typical Physical Characteristics

o

o

o

o

PHILLIPS66 VICTORY AW 20W-50 AVIATION OIL

* 제조사 :

* 모델명 :

Specifications, Approvals

& Recommendations

Phillips 66® Victory AW 20W-50 Oil is an ashless dispersant, multi-grade engine oil specially formulated for year-round use in aircraft piston engines. Victory AW 20W-50 is pre-blended with the proper concentration of antiscuff/antiwear additive (LW-16702) mandated by Lycoming Service Bulletins 446E and 471B and Service Instruction 1409C. It provides distinct performance benefits compared with single-grade engine oils, including easier starting and faster oil circulation at low temperatures, reduced warm-up time, and reduced oil consumption in most

engines.

Applications

Victory AW 20W-50 Aviation Oil is recommended for use in opposed piston engines. It can replace Commercial Grade 65, 80 or 100 single-grade engine oils with no sacrifice in performance.

Victory AW 20W-50 Oil meets the requirements of:

• Avco Lycoming Service Instruction 1014

• Pratt & Whitney Service Bulletin No. 1183 Rev. U

• SAE Standard J1899

• Teledyne Continental Material Specification MHS-24B

• U.S. Military Specification MIL-L-22851D (obsolete) for additive treatment QPL Approval Numbers:

Features/Benefits

• Ashless dispersant helps minimize engine sludge and varnish deposits for a cleaner engine

• Pre-blended with

Lycoming-approved antiwear additive

• Easier starting and faster oil circulation at low temperatures compared with single-grade oils

• Reduced warm-up time and cooler operating temperatures compared with single-grade oils

• High film strength for protection against wear and piston scuffing, even under high-load conditions, such as takeoff, and at elevated operating temperatures

• Protects against rust and corrosion

• Reduces oil consumption in most engines

• Suitable for year-round use

Typical Physical Characteristics

※ 입찰규격 확인서 작성 유의 사항

* 입찰 공고된 규격 기준과 일치하는 품목으로 구성되어야 함

- 공고된 규격 기준과 동일한 경우 비고란에 ‘공고 규격과 동일’ 표기

* 단종 등 불가피한 사유로 규격을 변경하여 제안하려는 경우에는 규격·품질·성능이 동등 이상인 품목으로 하며, 비고란에 사유 명시 및 입찰 참가 전 반드시 수요 부서에 확인을 받아야 함

- C-172(세스나 단발항공기) 정비교범에 의거 올바른 엔진오일 점도 규격에 일치하는 제품 사용 필요

* 입찰서 제출 시 본 입찰 규격 확인서를 반드시 첨부해야 함

* 수요 부서의 물품 규격 및 증빙서류 확인 결과, 동등 이상으로 인정되지 않는 경우에는 낙찰 후라도 선정을 취소하며, 입찰자는 이에 대한 이의를 제기할 수 없음